Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### RIP Administration Guide

Search Scope:

- This Document
- Entire Library

## Test the Default Metric

1. On switch 1, enter the configuration mode for the router.

       SEFOS# configure terminal
       SEFOS(config)# router rip
       SEFOS(config-router)# network 10.0.0.1

2. Set the default metric value (10 in this example).

       SEFOS(config-router)# default-metric 10

3. Configure the redistribution of static routes into the RIP domain.

       SEFOS(config-router)# redistribute static
       SEFOS(config-router)# exit

4. Add static routes.

       SEFOS(config)# ip route 50.0.0.0 255.0.0.0 vlan 2
       SEFOS(config)# ip route 60.0.0.0 255.0.0.0 vlan 2
       SEFOS(config)# ip route 70.0.0.0 255.0.0.0 vlan 2
       SEFOS(config)# ip route 80.0.0.0 255.0.0.0 vlan 2
       SEFOS(config)# end

5. On switch 2, test the default metric.

       SEFOS# show ip rip database

       10.0.0.0/8 [1] auto-summary
       10.0.0.0/16 [1] directly connected, vlan1
       50.0.0.0/8 [11] auto-summary
       50.0.0.0/8 [11] via 10.0.0.1, vlan1
       60.0.0.0/8 [11] auto-summary
       60.0.0.0/8 [11] via 10.0.0.1, vlan1
       70.0.0.0/8 [11] auto-summary
       70.0.0.0/8 [11] via 10.0.0.1, vlan1
       80.0.0.0/8 [11] auto-summary
       80.0.0.0/8 [11] via 10.0.0.1, vlan1

   Review the IP routing table.

       SEFOS# show ip route
       C 10.0.0.0/16 is directly connected, vlan1
       C 30.2.2.0/24 is directly connected, vlan3
       R 50.0.0.0/8 [11] via 10.0.0.1
       R 60.0.0.0/8 [11] via 10.0.0.1
       R 70.0.0.0/8 [11] via 10.0.0.1
       R 80.0.0.0/8 [11] via 10.0.0.1

6. On switch 1, review the metric for the redistributed RIP route entries.

       SEFOS# show ip protocols

       Routing Protocol is rip

       Vrf  default
        RIP2 security level is Maximum
        Redistributing : rip, static
        Output Delay is disabled
        Retransmission timeout interval is 5 seconds
        Number of retransmission retries is 36
        Default metric is 10
        Auto-Summarisation of routes is enabled
        Routing for Networks :
          10.0.0.0
        Routing Information Sources :
        Interface Specific Address Summarization :
        Trusted Neighors :
        Interface vlan1
         Sending updates every 30 seconds
         Invalid after 180 seconds
         Flushed after 120 seconds
         Send version is 1 2, receive version is 1 2
         Authentication type is none
         Split Horizon with poissoned reverse is enabled
         Restrcts default route installation
          Restricts default route origination

7. On switch 1, review the RIP configuration information.

       SEFOS# show ip rip database

       10.0.0.0/8  [1]        auto-summary
       10.0.0.0/16 [1]        directly connected, vlan1
       50.0.0.0/8  [10]        auto-summary
       50.0.0.0/8  [10]        redistributed via 0.0.0.0
       60.0.0.0/8  [10]        auto-summary
       60.0.0.0/8  [10]        redistributed via 0.0.0.0
       70.0.0.0/8  [10]        auto-summary
       70.0.0.0/8  [10]        redistributed via 0.0.0.0
       80.0.0.0/8  [10]        auto-summary
       80.0.0.0/8  [10]        redistributed via 0.0.0.0

8. On switch 1, disable redistribution.

       SEFOS# configure terminal
       SEFOS(config)# router rip
       SEFOS(config-router)# no redistribute static
       SEFOS(config-router)# end

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |