Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### IPv6 Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure Switch 2

1. Shut down the spanning tree.

       SEFOS# configure terminal
       SEFOS(config)# shutdown spanning-tree

2. Disable GVRP and GMRP.

       SEFOS(config)# set gvrp disable
       SEFOS(config)# set gmrp disable

3. Create the interface for `VLAN 2`, and enable IPv6.

       SEFOS(config)# interface vlan 2
       SEFOS(config-if)# shutdown
       SEFOS(config-if)# ipv6 enable
       SEFOS(config-if)# ipv6 address fec0::3333:0:1 96 unicast
       SEFOS(config-if)# no shutdown
       SEFOS(config-if)# exit

4. Create the P15 interface in `VLAN 2`.

       SEFOS(config)# vlan 2
       SEFOS(config-vlan)# ports extreme-ethernet 0/15 untagged extreme-ethernet 0/15
       SEFOS(config-vlan)# exit

5. Configure the extreme-ethernet interface.

       SEFOS(config)# interface extreme-ethernet 0/15
       SEFOS(config-if)# switchport pvid 2
       SEFOS(config-if)# no shutdown
       SEFOS(config-if)# exit

6. Enable IPv6 in `VLAN 3`.

       SEFOS(config)# interface vlan 3
       SEFOS(config-if)# shutdown
       SEFOS(config-if)# ipv6 enable
       SEFOS(config-if)# ipv6 address fec0::2222:0:10 96 unicast
       SEFOS(config-if)# no shutdown
       SEFOS(config-if)# exit

7. Create the P3 interface in `VLAN 3`.

       SEFOS(config)# vlan 3
       SEFOS(config-vlan)# ports extreme-ethernet 0/3 untagged extreme-ethernet 0/3
       SEFOS(config-vlan)# exit

8. Configure the extreme-ethernet interface.

       SEFOS(config)# interface extreme-ethernet 0/3
       SEFOS(config-if)# switchport pvid 3
       SEFOS(config-if)# no shutdown
       SEFOS(config-if)# end

9. Configure the IPv6 routing on switch 2.

       SEFOS# configure terminal
       SEFOS(config)# ipv6 route fec0::1111:0:0 96 fec0::2222:0:1
       SEFOS(config)# exit

10. Review the IPv6 information on switch 1.

        SEFOS# show ipv6 interface

        vlan1 is up, line protocol is up
            Link local address:
                fe80::201:2ff:fe03:501
            Global unicast address(es):
                fec0::1111:0:1/96
            Joined group address(es):
                ff02::1
                ff02::2
                ff02::1:ff00:1
                ff02::1:ff03:501
            MTU is 9216
            ICMP redirects are enabled
            ND DAD is enabled, Number of DAD attempts: 1
            ND router advertisement is disabled
        vlan3 is up, line protocol is up
            Link local address:
                fe80::201:2ff:fe03:501
            Global unicast address(es):
                fec0::2222:0:1/96
            Joined group address(es):
                ff02::1
                ff02::2
                ff02::1:ff00:1
                ff02::1:ff03:501
            MTU is 1500
            ICMP redirects are enabled
            ND DAD is enabled, Number of DAD attempts: 1
            ND router advertisement is disabled

11. Review the IPv6 routing table on switch 1.

        SEFOS# show ipv6 route

        IPv6 Routing Table:
        Codes : C - Connected, S - Static
                O - OSPF, R - RIP, B - BGP
        C   fec0::1111:0:0/96   [1/1]
                via ::, vlan1

        C   fec0::2222:0:0/96   [1/1]
                via ::, vlan3

        S   fec0::3333:0:0/96   [1/20]
                via fec0::2222:0:10, vlan3

12. Review the IPv6 information on switch 2.

        SEFOS# show ipv6 interface
        vlan1 is up, line protocol is up
            Link local address:
                fe80::202:2ff:fe03:401
            Global unicast address(es):
                Not Configured.
            Joined group address(es):
                ff02::1
                ff02::2
                ff02::1:ff03:401
            MTU is 1500
            ICMP redirects are enabled
            ND DAD is enabled, Number of DAD attempts: 1
            ND router advertisement is disabled
        vlan2 is up, line protocol is up
            Link local address:
                fe80::202:2ff:fe03:401
            Global unicast address(es):
                fec0::3333:0:1/96
            Joined group address(es):
                ff02::1
                ff02::2
                ff02::1:ff00:1
                ff02::1:ff03:401
            MTU is 1500
            ICMP redirects are enabled
            ND DAD is enabled, Number of DAD attempts: 1
            ND router advertisement is disabled
        vlan3 is up, line protocol is up
            Link local address:
                fe80::202:2ff:fe03:401
            Global unicast address(es):
                fec0::2222:0:10/96
            Joined group address(es):
                ff02::1
                ff02::2
                ff02::1:ff00:10
                ff02::1:ff03:401
            MTU is 1500
            ICMP redirects are enabled
            ND DAD is enabled, Number of DAD attempts: 1
            ND router advertisement is disabled

13. Review the routing table information in switch 2.

        SEFOS# show ipv6 route

        IPv6 Routing Table:
        Codes : C - Connected, S - Static
                O - OSPF, R - RIP, B - BGP
        S   fec0::1111:0:0/96   [1/20]
                via fec0::2222:0:1, vlan3

        C   fec0::2222:0:0/96   [1/1]
                via ::, vlan3

        C   fec0::3333:0:0/96   [1/1]
                via ::, vlan2

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |