Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### XVLAN Administration Guide

Search Scope:

- This Document
- Entire Library

#### Multiple-Switch Topology

A typical XVLAN configuration has multiple switches, interconnected with VLAN trunks. The example configuration in this section illustrates how to interconnect two SEFOS switches (SEFOS1 and SEFOS2), and extend the XVLAN across them. There are two restricted XVLANs on these switches under principal XVLAN 100.

This figure shows the IP addresses and port assignments for the multiple-switch configuration. In this example, port 1 is the external port on both switches (SEFOS1 and SEFOS2). On SEFOS1, ports 19 and 20 are solitary-restricted internal ports, and ports 2 and 15 are group-restricted internal ports. On SEFOS2, ports 11 and 12 are solitary-restricted internal ports. Port 2 is the only group-restricted internal port.

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |