Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### LA Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the LACP Wait Time

The LACP wait time is the interval of time the system takes to aggregate a link. Configuring the wait time value as 0 ensures that links get aggregated immediately. The default value for the LACP wait time is 2.

1. Enter the configuration mode for the interface (0/1 in this example).

       SEFOS(config)# configure terminal
       SEFOS(config)# interface extreme-ethernet 0/1

2. Configure the LACP wait time.

       SEFOS(config-if)# lacp wait-time 1

3. Review the `etherchannel` information.

       SEFOS# show etherchannel 1 detail
       ...
       LACP port-priority  = 128
       LACP Wait-time  = 1 secs
       LACP Port Identifier = 1
       ...

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |