Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### IGMP Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the IGMP Last Member Query Interval

1. Enter Interface Configuration mode for `VLAN 2`.

       SEFOS# configure terminal
       SEFOS(config)# interface vlan 2

2. Set the last member query interval to 20 seconds.

       SEFOS(config-if)# ip igmp last-member-query-interval 20
       SEFOS(config-if)# end

3. Ensure that the query interval has changed.

       SEFOS# show ip igmp interface vlan 2
       ...
       Last member query response interval is 20 seconds
       ...

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |