Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### LA Administration Guide

Search Scope:

- This Document
- Entire Library

## Enable Link Aggregation

LA is disabled by default. See LA Topology Example for the topology of this procedure.

1. In both switches, enable LA.

       SEFOS# configure terminal
       SEFOS(config)# set port-channel enable
       SEFOS(config)# end

2. View the `etherchannel` information.

       SEFOS# show etherchannel summary

   The output in switch A and switch B should be:

       Port-channel Module Admin Status is enabled
       Port-channel Module Oper Status is enabled
       Port-channel System Identifier is  00:14:4f:6c:68:2f

   Note - To shut down the entire LA module, type the `shutdown port-channel` command.

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |