Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### SLB Administration Guide

Search Scope:

- This Document
- Entire Library

#### Dual-Switch Configuration

This example shows a dual-switch configuration, with the servers configured in between the two switches as the "bump". Each server is dual homed. LBG are formed in a symmetric way (LBG on each switch has the same port members setup in the exact same order).

Feature | Example Setting
--- | ---
Group ID | 1
Switch port for server 1 | extreme-ethernet 0/15 on switch 2
Switch port for server 2 | extreme-ethernet 0/16 on switch 2
Switch port for server 3 | extreme-ethernet 0/17 on switch 2
Switch port for server 4 | extreme-ethernet 0/18 on switch 2

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |