Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPFv3 Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuring the Capability in an NSSA Internal Border Router

Configuring the p-bit in the Type-7 LSA allows the Type-7 LSA to get converted into a Type-5 LSA by the NSSA ABR, or to not to convert it. Type-7 LSAs are generated from an AS-external border router that contains the routing information about the external AS link RIPng, BGP, and the like.

- Configure NSSA Type-7/-5 Conversion

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |