Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPFv3 Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the Neighbor Probe Interval

This example specifies that the neighbor will be probed every 130 seconds.

1. Configure the neighbor probe interval for the specified interface.

       SEFOS(config)# interface vlan 10
       SEFOS(config-if)# ipv6 ospf demand-circuit
       SEFOS(config-if)# ipv6 ospf neighbor-probe interval 130

2. Ensure that the specified interface will be probed at the correct interval.

       SEFOS# show ipv6 ospf interface vlan 10

               Ospfv3  Interface  Information

       Interface Name: vlan10      Interface Id: 41    Area Id: 0.0.0.6
       Local Address: fe80::214:4fff:fe6c:628f         Router Id: 10.0.0.1
       Network Type: BROADCAST     Cost: 1             State: BACKUP
       Designated Router Id: 10.0.0.8      local address: fe80::214:4fff:fe6c:d04d
       Backup Designated Router Id: 10.0.0.1      local address: fe80::214:4fff:fe6c:628f
       Transmit Delay: 1 sec        Priority: 1         IfOptions: 0x0
       Timer intervals configured:
       Hello: 10, Dead: 40, Retransmit: 5, Poll: 120
       Demand Circuit: Enable             Neighbor Probing: Enable
       Nbr Probe Retrans Limit: 10        Nbr Probe Interval: 130
       Hello due in 2 sec
       Neighbor Count is: 1
       Adjacent with neighbor 10.0.0.8

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |