Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### IPv6 Administration Guide

Search Scope:

- This Document
- Entire Library

### Basic SEFOS IPv6 Topology

This illustration depicts a basic Oracle's SEFOS IPv6 topology that is referenced in this guide. In this topology, two switches (switch 1 and switch 2) are connected to each other over port 0/3 (P3). Host A and host B are connected through port 0/1 to their respective switches. Finally, three VLANs are enabled. `VLAN 3` connects the two switches, and `VLAN 1` and `VLAN 2` connect the hosts to the switches.

The following table lists the IPv4 and IPv6 addresses of the interfaces and hosts shown in the example topology.

Switch or Host | Interface | IPv4 Address and Mask | IPv6 Address and Prefix Length
--- | --- | --- | ---
Switch 1 | `VLAN 1` | `11.0.0.1` / `255.0.0.0` | `fec0::1111:0:1` / `96`
`VLAN 3` | `22.0.0.1` / `255.0.0.0` | `fec0::2222:0:1` / `96`
Switch 2 | `VLAN 2` | `33.0.0.1` / `255.0.0.0` | `fec0::3333:0:1` / `96`
`VLAN 3` | `22.0.0.1` / `255.0.0.0` | `fec0::2222:0:10` / `96`
Host A |  | `11.0.0.1` / `255.0.0.0` | `fec0::1111:0:10` / `96`
Host B |  | `33.0.0.1` / `255.0.0.0` | `fec0::3333:0:10` / `96`

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |