Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### DHCP Administration Guide

Search Scope:

- This Document
- Entire Library

## Enable the Relay Agent Information

1. Enable the relay agent information option in switch 2.

       SEFOS# configure terminal
       SEFOS(config)# ip dhcp relay information option
       SEFOS(config)# end

2. View the relay agent information status.

       SEFOS# show ip dhcp relay information

   The output in the switch is:

       Dhcp Relay                                   : Enabled
       Dhcp Relay Servers only                  : Enabled

       DHCP server                                 : 20.0.0.1

       Dhcp Relay RAI option                    : Enabled
       Default Circuit Id information             : router-index
       Debug Level                                  : 0x1

       No of Packets inserted RAI option               : 0
       No of Packets inserted circuit ID suboption     : 0
       No of Packets inserted remote ID suboption      : 0
       No of Packets inserted subnet mask suboption    : 0
       No of Packets dropped                           : 0
       No of Packets which did not inserted RAI option : 0

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |