Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPF Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuring the NSSA Area, Summary Address, and Area Default Cost

These sections explain how to configure the NSSA area, summary address, and area default cost.

- NSSA Configuration, Summary Address Configuration, and Area Default-Cost

- Configure the NSSA Area

- Reconfigure Area `0.0.0.6` as a Normal Area

- Configure the Summary Address

- Delete the Summary Address Configuration for `90.0.0.0/8` in the NSSA Area

- Configure the Area Default Cost

- Configure Default-Cost for the Default Summary Route Sent Into the NSSA Area

- Configure SEFOS2

- Configure SEFOS4

- Configure SEFOS9

- Examine the Configuration Details in SEFOS2

- Examine the Configuration Details in SEFOS4

- Examine the Configuration Details in SEFOS9

- Test SEFOS9

- Test SEFOS2

- Test SEFOS9

- Configure the P-bit Setting in the Default Type 7 LSA

- Disable the P-bit Setting in the Default Type 7 LSA

- Configure the NSSA Area Translation Role

- Configure the Stability Interval for NSSA

- Configure the ABR Type

- Configure RFC 1583 Compatibility

- Disable RFC 1583 Compatibility

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |