Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PIMv6 Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the Query-Interval Value

The query-interval value enables PIMv6 on an interface, and sets the frequency at which PIMv6 hello messages are transmitted on the interface.

1. Associate the `VLAN 7` interface with PIMv6 component 1.

       SEFOS(config)# interface vlan 7
       SEFOS(config-if)# ipv6 pim componentId 1
       SEFOS(config-if)# end

2. Set the query interval to 60 seconds for the `VLAN 7` interface.

       SEFOS# configure terminal
       SEFOS(config)# interface vlan 7
       SEFOS(config-if)# ipv6 pim query-interval 60
       SEFOS(config-if)# end

3. Review the PIMv6 query interval.

       SEFOS# show ipv6 pim interface detail

       vlan7 34 is up
       ...
           PIM Hello/Query Interval : 60
       ...

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |