Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPF Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the Area Range

Area range is configured to consolidate and summarize routes at an area boundary.

1. Type.

       SEFOS# configure terminal
       SEFOS(config)# router ospf

2. Configure the OSPF router ID.

       SEFOS(config-router)# router-id 10.10.2.1

3. Configure the OSPF interface.

       SEFOS(config-router)# network 10.4.0.1 area 0.0.0.0
       SEFOS(config-router)# network 10.10.2.1 area 0.0.0.6

4. Configure the route summarization at an area border router.

       SEFOS(config-router)# area 0.0.0.6 range 10.10.0.0 255.255.0.0 summary

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |