Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### IGMP Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the IGMP Query Interval

1. Enter Interface Configuration mode for `VLAN 2`.

       SEFOS# configure terminal
       SEFOS(config)# interface vlan 2

2. Set the IGMP query interval to 200 seconds.

       SEFOS(config-if)# ip igmp query-interval 200
       SEFOS(config-if)# end

3. Review the query interval information.

       SEFOS# show ip igmp interface vlan 2

       ...
       IGMP query interval is 200 seconds
       ...

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |