Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PVRST+ Administration Guide

Search Scope:

- This Document
- Entire Library

#### Bridge ID and Switch Priority

Each switch has a unique bridge identifier (bridge ID), that determines the selection of the root switch. The bridge ID is an 8-byte field that is composed of two sub fields:

The value for the priority ranges from 0 to 61440 in steps of 4096. The default value for the priority is 32768. The VLAN ID ranges from 1 to 4096.

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |