Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### DHCP Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure a DHCP Server Address

You can configure a DHCP server address in the DHCP relay agent. A maximum of five servers can be configured. If no servers are configured, the DHCP packets will be broadcast to the entire network, except to the network from which the packet is received.

In this example, the server address is `20.0.0.1`.

1. Configure a DHCP server address in switch 2.

       SEFOS# configure terminal
       SEFOS(config)# ip dhcp server 20.0.0.1
       SEFOS(config)# end

2. Ensure that the server address has been configured in the relay.

       SEFOS# show ip dhcp relay information

   The output in the switch is:

       Dhcp Relay                                   : Enabled
       Dhcp Relay Servers only                  : Enabled

       DHCP server                                 : 20.0.0.1

       Dhcp Relay RAI option                    : Disabled
       Default Circuit Id information             : router-index
       Debug Level                                  : 0x1

       No of Packets inserted RAI option               : 0
       No of Packets inserted circuit ID suboption     : 0
       No of Packets inserted remote ID suboption      : 0
       No of Packets inserted subnet mask suboption    : 0
       No of Packets dropped                           : 0
       No of Packets which did not inserted RAI option : 0

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |