Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### MLDS Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuring Fast-Leave Processing

You can configure fast-leave processing to remove the interface from the forwarding table as soon as a leave message is received by the switch on that interface, without the switch sending MAC-based general queries to the interface. The VLAN interface is pruned from the multicast tree for the multicast group specified in the original leave message.

Immediate-leave processing ensures optimal bandwidth management for all hosts on a switched network, even when multiple multicast groups are simultaneously in use.

- Enable Fast-Leave Processing

- Disable Fast-Leave Processing

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |