Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PIM Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuring BSR Candidates

A BSR is a dynamically elected router within a PIM domain that enables routers to learn RP information. To specify which router is used as the BSR, you can assign a value for the local interface as a candidate BSR. The router with the highest priority value is used as the BSR. If two or more routers have the same priority value, the router with the largest IP address becomes the BSR.

- Prioritize BSR Candidates

- Restore the Default BSR-Candidate Value

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |