Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPFv3 Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuring a Stub Area

If an area is configured as a stub area, you can inject summary routes into it. You can also configure other parameters related to that area.

In a stub area, the generation of summary LSAs is optional. If you specify the `no-summary` option, the router will not propagate summary LSAs. By default, the stub area sends summary information.

You can configure area parameters only after enabling the OSPF process. Configure these parameters in Router Configuration mode.

- Configure a Stub Area

- Convert a Stub Area to a Normal Area

- Configure a Default Summary Route for a Stub Area

- Configure the Default Summary Route Cost for a Stub Area

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |