Go to main content
oracle home
Sun Network 10GbE Switch 72p Product Notes

Exit Print View

Search Term
Search Scope:
This Document Entire Library
Updated: November 2016

- Sun Network 10GbE Switch 72p Product Notes
- Document Information
- Using This Documentation

- Product Documentation Library
- Feedback

- Late-Breaking Information

- Switch Documentation Reading Order
- New Features

- IPv6 Switching and Routing
- PVRST+ Protocol
- Exclusive VLAN
- Data Center Bridging
- Internet Group Management Protocol
- PIM
- Q-in-Q Tunneling
- Server Load Balancer Layer 3
- Uplink Port Trailing
- VRRPv3
- Oracle ILOM 3.0 Features

- Enhancements
- Upgrading the Switch Firmware

- Back Up the Current Configuration Before Upgrading
- Download the Switch Firmware Package
- Install the Switch Updates

- Configuring the Switch

- Configure 1Gbps Mode on SFP+ Interfaces
- Fine Tune the VLAN Setup
- Managing SEFOS Configurations

- Include the SEFOS Configuration in Backups
- Restore the Configuration

- Configuring TACACS+

- TACACS+ Properties
- Configure TACACS+ Settings

- Known Issues

- Manually Deleting Static Routes Does Not Affect the Corresponding SLB Entry (7123134)
- PIMv6-SSM Mode is Not Supported in This Release (7114280)
- Firmware Upgrade With the Web UI is Incomplete (7022295)
- Changing the Default Value for default-vlan-id Could Result in VLAN Misconfiguration (7015004)
- Some of the IGMP Conformance Results Do Not Match Expectations (7006297 and 6997415)
- QoS - set algo-type tailDrop queue-drop-algo Does Not Work (6991230)
- Packets Might Be Dropped When Using Q-in-Q Interop in Certain Configurations (6989048)
- The no default-metric [,short(1-16)>] Command Does Not Work as Documented (6987482)
- Using vlan 1 as Shown in Various Examples in the Documentation Generates Error Codes (6968484)
- When Multiple Configuration Scripts Are Run in Parallel, SEFOS Can Crash (6936742)
- The switch Command Line Option Is Unsupported
- vrrp_v3: Role is incorrect for vlan with no premempt configuration after save/reboot (19547263)
- SSL V3.0 POODLE DISABLE SSL V3 (19842635)
- Re-configure IP address after a "no ip address", previous config re-appears (18794861)

Language:

### Fine Tune the VLAN Setup

The switch provides flexibility in managing ingress VLAN traffic. For example, you can set port ingress filtering to enabled and can also specify the acceptable frame type to implement fine-grained control on the ingress traffic. Refer to the Sun Ethernet Fabric Operating System CLI Base Reference Manual for details.

1. Obtain the SEFOS prompt.
2. Display the default port configuration.

       SEFOS# show vlan port config port extreme-ethernet 0/3

       Vlan Port configuration table
       -------------------------------
       Port Ex0/3
       Port Vlan ID                        : 1
       Port Acceptable Frame Type          : Admit All
       Port Ingress Filtering              : Disabled
       Port Mode                           : Hybrid
       Port Gvrp Status                    : Enabled
       Port Gmrp Status                    : Enabled
       Port Gvrp Failed Registrations      : 0
       Gvrp last pdu origin                : 00:00:00:00:00:00
       Port Restricted Vlan Registration   : Disabled
       Port Restricted Group Registration  : Disabled
       Mac Based Support                   : Disabled
       Subnet Based Support                : Disabled
       Port-and-Protocol Based Support     : Enabled
       Default Priority                    : 0
       Filtering Utility Criteria          : Default
       Port Protected Status               : Disabled
       -------------------------------------------------------

3. Reconfigure the port.

   For example, to reconfigure the 10GbE port Ex0/3 as a tagged port in vlan 3 and allowing only tagged frames:

       SEFOS# config terminal
       SEFOS(config)# vlan 3
       SEFOS(config-vlan)# port extreme-ethernet 0/3
       SEFOS(config-vlan)# exit
       SEFOS(config)# interface extreme-ethernet 0/3
       SEFOS(config-if)# switchport ingress-filter
       SEFOS(config-if)# switchport acceptable-frame-type tagged
       SEFOS(config-if)# end
       SEFOS# show vlan port config port extreme-ethernet 0/3

       Vlan Port configuration table
       -------------------------------
       Port Ex0/3
       Port Vlan ID                        : 1
       Port Acceptable Frame Type          : Admit Only Vlan Tagged
       Port Ingress Filtering              : Enabled
       Port Mode                           : Hybrid
       Port Gvrp Status                    : Enabled
       Port Gmrp Status                    : Enabled
       Port Gvrp Failed Registrations      : 0
       Gvrp last pdu origin                : 00:00:00:00:00:00
       Port Restricted Vlan Registration   : Disabled
       Port Restricted Group Registration  : Disabled
       Mac Based Support                   : Disabled
       Subnet Based Support                : Disabled
       Port-and-Protocol Based Support     : Enabled
       Default Priority                    : 0
       Filtering Utility Criteria          : Default
       Port Protected Status               : Disabled

4. Add an untagged port.

   - To use the preferred method, go to Step 5.

   - To use the alternate method, go to Step 6.

5. Add an untagged port using the preferred method.
   1. Type these commands.

      For example, add 10GbE port Ex0/3 to vlan 3 as untagged.

          SEFOS# configure terminal
          SEFOS(config)# interface extreme-ethernet 0/3
          SEFOS(config-if)# switchport access vlan 3
          SEFOS(config-if)# end

   2. Verify the port VLAN ID.

          SEFOS# show vlan port config port extreme-ethernet 0/3

          Vlan Port configuration table
          -------------------------------
          Port Ex0/3
           Port Vlan ID                        : 3
           Port Acceptable Frame Type          : Admit All
           Port Ingress Filtering              : Enabled
           Port Mode                           : Hybrid
           Port Gvrp Status                    : Disabled
           Port Gmrp Status                    : Disabled
           Port Gvrp Failed Registrations      : 0
           Gvrp last pdu origin                : 00:00:00:00:00:00
           Port Restricted Vlan Registration   : Disabled
           Port Restricted Group Registration  : Disabled
           Mac Based Support                   : Disabled
           Subnet Based Support                : Disabled
           Port-and-Protocol Based Support     : Enabled
           Default Priority                    : 0
           Dot1x Protocol Tunnel Status        : Peer
           LACP Protocol Tunnel Status         : Peer
           Spanning Tree Tunnel Status         : Peer
           GVRP Protocol Tunnel Status         : Peer
           GMRP Protocol Tunnel Status         : Peer
           IGMP Protocol Tunnel Status         : Peer
           Filtering Utility Criteria          : Default
           Port Protected Status               : Disabled

6. Add an untagged port using the alternate method.
   1. Type these commands.

      For example, add 10GbE port Ex0/4 to vlan 4 as untagged.

          SEFOS# configure terminal
          SEFOS(config)# vlan 4
          SEFOS(config-vlan)# ports extreme-ethernet 0/4 untagged extreme-ethernet 0/4
          SEFOS(config-vlan)# exit
          SEFOS(config)# interface extreme-ethernet 0/4
          SEFOS(config-if)# switchport pvid 4
          SEFOS(config-if)# end

   2. Verify the port VLAN ID.

          SEFOS# show vlan port config port extreme-ethernet 0/4

          Vlan Port configuration table
          -------------------------------
          Port Ex0/4
           Port Vlan ID                        : 4
           Port Acceptable Frame Type          : Admit All
           Port Ingress Filtering              : Enabled
           Port Mode                           : Hybrid
           Port Gvrp Status                    : Disabled
           Port Gmrp Status                    : Disabled
           Port Gvrp Failed Registrations      : 0
           Gvrp last pdu origin                : 00:00:00:00:00:00
           Port Restricted Vlan Registration   : Disabled
           Port Restricted Group Registration  : Disabled
           Mac Based Support                   : Disabled
           Subnet Based Support                : Disabled
           Port-and-Protocol Based Support     : Enabled
           Default Priority                    : 0
           Dot1x Protocol Tunnel Status        : Peer
           LACP Protocol Tunnel Status         : Peer
           Spanning Tree Tunnel Status         : Peer
           GVRP Protocol Tunnel Status         : Peer
           GMRP Protocol Tunnel Status         : Peer
           IGMP Protocol Tunnel Status         : Peer
           Filtering Utility Criteria          : Default
           Port Protected Status               : Disabled

Previous
Next