Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPFv3 Administration Guide

Search Scope:

- This Document
- Entire Library

### Default Configuration Values

By default, OSPFv3 and IPv6 addressing are disabled on a switch running SEFOS. To configure an OSPFv3 router or to configure an interface with an IPv6 address, you must first enable OSPFv3 or IPv6 on the interfaces.

Parameter | Default Configuration
--- | ---
`ABR-type` | Standard
`Area default-cost` | 10
Area metric value | 1
Area type | Transit
`AS-external LSDB-limit` | -1 (no limit)
`Dead-interval` | 40
Default network type | Broadcast
Default OSPFv3 trace level | Critical (If enabled)
Default-information originate always metric | 10
Default-information originate always metric-type | 2
Demand circuit | Enabled
Exit overflow interval | 0
Hello-interval | 10
IETF non-stop forwarding | Disabled
IETF NSF helper strict LSA check | Disabled
IETF NSF helper support unknown/s/w restart/s/w upgrade/ switch to redundant | Enabled
Interface metric | From the reference bandwidth
IPv6 on the interface | Disabled
Neighbor-probe retransmit - interval | 120
Neighbor-probe retransmit-limit | 10
nssa asbr-default-route translator | Disabled
OSPFv3 module on the router | Disabled
OSPFv3 traces | Disabled
Passive interface | Disabled
Poll-interval | 120
Redist-config metric-type | Type-2
Redist-config metric-value | 10
Redist-config tag | 0
Reference bandwidth | 100000
Retransmit-interval | 5
Route calculation staggering | Enabled
Router priority | 1
SPF hold time | 10
SPF timer delay | 5
Stability interval | 40
Staggering interval | 10
Summary-address | Advertise
Translation | Enabled
Translation-role | Candidate
Transmit-delay | 1

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |