Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### MLDS Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the Snooping Version

The snooping version for a specific VLAN can be configured as either v1 or v2. By default, the operating version of the MLDS switch for all the VLANs is v2. In this example, `VLAN 4` is the VLAN for which the snooping version is to be configured, and the snooping version is `1`.

1. Configure the snooping version.

       SEFOS# configure terminal
       SEFOS(config)# vlan 4
       SEFOS(config-vlan)# ipv6 mld snooping version v1
       SEFOS(config-vlan)# end

2. View the configuration.

       SEFOS# show ipv6 mld snooping vlan 4

       Snooping VLAN Configuration for the VLAN 4
         MLD Snooping enabled
         MLD configured version is V1
         Fast leave is disabled
         Snooping switch is configured as Non-Querier
         Snooping switch is acting as Non-Querier
         Query interval is 125 seconds
         Port Purge Interval is 260 seconds
         Max Response Code is 10000, Time is 10 seconds

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |