Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PIMv6 Administration Guide

Search Scope:

- This Document
- Entire Library

## Global Configurations

This section contains procedures for configuring the Oracle's SEFOS PIMv6 features. The configurations are global to all of the components in a router. Some of these procedures have the default values shown in Default Settings. You do not need to reconfigure these values unless your administration requirements are different.

Note - In some procedures in this section, the example output has been truncated for readability.

- Enable PIMv6

- Configure the Group and Source Thresholds

- Configure the SPT Switching Period

- Configure the Rendezvous Point Threshold

- Configure the RP Switch Period

- Configure the regstop Rate Limit

- Configure the PMBR Status

- Configuring PIMv6 on an Interface

- Configuring the PIMv6 Component

- Create a PIMv6 Neighbor

- Create Multicast Routes

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |