Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PIM Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuring PIM Join and Prune Messaging

You can specify the frequency with which PIM join and prune messages are transmitted on a PIM interface. The join and prune message interval used must be the same on all PIM routers in the PIM domain. If all the routers do not use the same timer interval, then the performance of PIM sparse can be adversely affected.

- Specify the Join and Prune Messaging Interval

- Restore the Default Message Interval

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |