Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPFv3 Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure All Interfaces To Be Passive

If you want to configure all interfaces to be passive, you must do so before you create the interfaces.

1. Enable OSPF globally in SEFOS1.

       SEFOS(config)# ipv6 router ospf

2. Suppress routing updates.

       SEFOS(config-router)# passive-interface
       SEFOS(config-router)# end

3. Configure the interface, then view the modified configuration.

       SEFOS# show ipv6 ospf interface vlan 10

               Ospfv3  Interface  Information

       Interface Name: vlan10      Interface Id: 41    Area Id: 0.0.0.6
       Local Address: fe80::214:4fff:fe6c:628f         Router Id: 10.0.0.1
       Network Type: BROADCAST     Cost: 1             State: DR
       Designated Router Id: 10.0.0.1      local address: fe80::214:4fff:fe6c:628f
       Backup Designated Router Id: 0.0.0.0       local address: (null)
       Transmit Delay: 1 sec        Priority: 1         IfOptions: 0x0
       Timer intervals configured:
       Hello: 10, Dead: 40, Retransmit: 5, Poll: 120
       Demand Circuit: Disable            Neighbor Probing: Disable
       Nbr Probe Retrans Limit: 10        Nbr Probe Interval: 120
       No Hellos (Passive interface)
       Neighbor Count is: 0

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |