Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### LLDP Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuration Topology

All the configurations explained in this document are based on the following topology.

Switch 1 has the following configuration:

- Interface P1 exists and is operational.

- MAC address is `00:01:02:03:04:01`.

- Default default IP address for the VLAN is `12.0.0.1`.

Switch 2 has the following configuration:

- Interface P1 exists and is operational.

- MAC address is `00:02:02:03:04:01`.

  You can also use the preconfigured MAC address.

- Default VLAN IP address is `12.0.0.2`.

Copyright © 2010, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |