Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPFv3 Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure a Stub Area

This example configures the IP address `0.0.0.6` as a stub area in SEFOS1 (router ID `10.0.0.1`).

1. Enter Global Configuration mode in SEFOS1.

       SEFOS# configure terminal

2. Enable OSPF globally in SEFOS1.

       SEFOS(config)# ipv6 router ospf

3. Configure the OSPF router ID.

       SEFOS(config-router)# router-id 10.0.0.1

4. Configure the desired area associated with the OSPF address range as a stub area.

       SEFOS(config-router)# area 0.0.0.6 stub
       SEFOS(config-router)# end

5. Ensure that the stub area is created.

       SEFOS# show ipv6 ospf areas

       OSPFV3  AREA  CONFIGURATION  INFORMATION
       AreaId: 0.0.0.0                 Area Type: NORMAL AREA
       Spf Calculation: 4 (times)      Area Bdr Rtr Count: 0
       As Bdr Rtr Count: 0             Area Summary: Send Summary

       AreaId: 0.0.0.6                 Area Type: STUB AREA
       Spf Calculation: 4 (times)      Area Bdr Rtr Count: 0
       As Bdr Rtr Count: 0             Area Summary: Send Summary
       Stub Metric: 0x1                Stub Metric Type: 1

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |