Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### IGMP Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure a Static-Multicast Group Membership

1. Enter Interface Configuration mode for `VLAN 2`.

       SEFOS# configure terminal
       SEFOS(config)# interface vlan 2

2. Add a static entry (`224.1.0.1`) for the multicast group.

       SEFOS(config-if)# ip igmp static-group 224.1.0.1
       SEFOS(config-if)# end

3. Ensure that the multicast groups joined.

       SEFOS# show ip igmp interface

       ...
        Number of multicast groups joined 1

4. Review the IGMP group information.

       SEFOS# show ip igmp groups

       I - Include Mode,  E - Exclude Mode
       S - Static Mbr,    D - Dynamic Mbr

       GroupAddress Flg Iface UpTime    ExpiryTime         LastReporter
       --------------- --- ------- ---------------- ---------------- ----
       224.1.0.1    ES  vlan2  [0d 00:00:22.12] [0d 00:00:00.00] 0.0.0.0

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |