Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### RIP Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure Basic Timers

1. On switch 1, enter the configuration mode for the interface.

       SEFOS# configure terminal
       SEFOS(config)# interface vlan 1
       SEFOS(config-if)# exit

2. Enter the configuration mode for the router.

       SEFOS# configure terminal
       SEFOS(config)# router rip
       SEFOS(config-router)# network 10.0.0.1
       SEFOS(config-router)# exit

3. Set the timers.

       SEFOS(config)# interface vlan 1
       SEFOS(config-if)# timers basic 60 120 120
       SEFOS(config-if)# end

4. Review the RIP update packets that are sent after 60 seconds and the configured timer values.

       SEFOS# show ip protocols

       Routing Protocol is rip

       Vrf  default
        RIP2 security level is Maximum
        Redistributing : rip, bgp, connected, ospf, static
        Output Delay is disabled
        Retransmission timeout interval is 5 seconds
        Number of retransmission retries is 36
        Default metric is 3
        Auto-Summarisation of routes is disabled
        Routing for Networks :
          10.0.0.0
        Routing Information Sources :
        Interface Specific Address Summarization :
          40.0.0.0/8    for vlan1
        Trusted Neighors :
        Interface vlan1
         Sending updates every 60 seconds
         Invalid after 120 seconds
         Flushed after 120 seconds
         Send version is 1 2, receive version is 1 2
         Authentication type is none
         Split Horizon with poissoned reverse is enabled
         Installs default route received
         Restricts default route origination

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |