Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPFv3 Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure Interface Priority

You can set the router priority to help determine the designated router for a given network. Values are 1-255, with a value of 0 signifying that the router is not eligible to become the designated router on a particular network.

This example configures `VLAN 10` with an interface priority of 10.

1. Configure the interface priority through the CLI.

       SEFOS(config)# interface vlan 10
       SEFOS(config-if)# ipv6 ospf priority 10
       SEFOS(config-if)# end

2. View the configuration.

       SEFOS# show ipv6 ospf interface vlan 10

               Ospfv3  Interface  Information
       Interface Name: vlan10      Interface Id: 41    Area Id: 0.0.0.6
       Local Address: fe80::214:4fff:fe6c:628f         Router Id: 10.0.0.1
       Network Type: BROADCAST     Cost: 1             State: BACKUP
       Designated Router Id: 10.0.0.8      local address: fe80::214:4fff:fe6c:d04d
       Backup Designated Router Id: 10.0.0.1      local address: fe80::214:4fff:fe6c:628f
       Transmit Delay: 1 sec        Priority: 10        IfOptions: 0x0
       Timer intervals configured:
       Hello: 10, Dead: 40, Retransmit: 5, Poll: 120
       Demand Circuit: Disable            Neighbor Probing: Disable
       Nbr Probe Retrans Limit: 10        Nbr Probe Interval: 120
       Hello due in 0 sec
       Neighbor Count is: 1
       Adjacent with neighbor 10.0.0.8

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |