Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PIM Administration Guide

Search Scope:

- This Document
- Entire Library

## Enable PMBR Status Reporting

PMBR status reporting is disabled by default.

This example enables PMBR status for `VLAN 5`. In addition, the PIM component is configured in the router as component 1.

1. Enable the PMBR status feature.

       SEFOS# configure terminal
       SEFOS(config)# set ip pim enable
       SEFOS(config)# set ip pim pmbr enable

2. Associate the interface with PIM component 1.

       SEFOS# interface vlan 5
       SEFOS(config-if)# ip pim componentId 1
       SEFOS(config-if)# end

3. View the PMBR status.

       SEFOS# show ip pim interface detail

       Vlan5 33 is up
         Internet Address is 10.1.0.1
         Muticast Switching : Enabled
         PIM : Enabled
         PIMv6 : Disabled
           PIM version : 2, mode: Sparse
           PIM DR : 10.1.0.1
           PIM DR Priority : 1
           PIM Neighbour Count : 0
           PIM Hello/Query Interval : 30
           PIM Message Interval : 60
           PIM Override Interval : 0
           PIM Lan Delay : 0
           PIM Lan-Prune-Delay : Disabled
           PIM Component Id : 1
           PIM domain border : enabled

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |