Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PIM Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuring PIM LAN Delay

The LAN delay expresses the expected message propagation delay on the interface. Upstream routers use this delay to determine the delayed time interval for a Join override message before pruning an interface.

- Delay LAN Message Propagation

- Restore the Default LAN Delay Interval

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |