Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### RIPng Administration Guide

Search Scope:

- This Document
- Entire Library

## Disable the `split-horizon` Option

By default, the `split-horizon` option with poison reverse is enabled on all RIPng interfaces.

1. On SEFOS1, enter the configuration mode for the interface and disable split-horizon.

       SEFOS 1 SEFOS# configure terminal
       SEFOS 1 SEFOS(config)# interface vlan 40
       SEFOS 1 SEFOS(config-if)# no ipv6 split-horizon
       SEFOS 1 SEFOS(config-if)# end
       SEFOS 1 SEFOS#

2. Review the configuration information.

       SEFOS 1 SEFOS# show ipv6 rip

       RIP  port 521, multicast-group ff02::9,Maximum paths is 16
       Updates every 30 seconds; expire after 180
       Garbage Collect after  120 seconds
       Split Horizon is off;
       Interface:
       vlan50
       vlan40
       vlan30
       Redistribution:
        Connected,Routes  Redistribution is enabled.

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |