Skip Navigation Links
Exit Print View
| Oracle Ethernet Switches ### L2 and L3 Deployment Best Practices

Search Scope:

- This Document
- Entire Library

### Sun Blade 6000 Ethernet Switched NEM 24p 10GbE

Sun Blade 6000 Ethernet Switched NEM 24p 10GbE is a multipurpose connectivity module for the Sun Blade 6000 modular system. The NEM supports connection to external devices through 10GbE SFP+ ports and QSFP ports. The NEM connects server modules (blades) in a Sun Blade 6000 modular system chassis with disk modules in the same chassis.

For installation, configuration, and management information, refer to the documentation at: http://www.oracle.com/goto/SB6K-24p-10GbE/docs

##### Additional L2 and L3 Configurations for Sun Blade 6000 Ethernet Switched NEM 24p 10GbE

For the following configurations, refer to the Sun Blade 6000 Ethernet Switched NEM 24p 10GbE Software Configuration Guide at: http://www.oracle.com/goto/SB6K-24p-10GbE/docs

- Switching Feature

  - VLAN Forwarding

  - RSTP

  - LA

- Routing Feature

  - Static Unicast Route Entries

  - Dynamic Routing with RIP

  - Dynamic Routing with OSPF

- Topology – SFP+ LAG and Backplane Portface Connection

- Topology – Layer 2 Switch LAG and QSFP Splitter SAN Connection

- Topology – Switched NEM High Availability Connection

  - Four NEM/Two Chassis High Availibility

- Topology – Four Switched NEMs, High Availability Connection

  - Four NEM/Four Chassis High Availibility

  - QSFP Ports Into a Link Aggregation

##### Related Information

- Oracle Switch ES1-24

- Sun Network 10GbE Switch 72p

Copyright © 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |