Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### RIP Administration Guide

Search Scope:

- This Document
- Entire Library

## Disable the RIP Passive Interface

1. On switch 1, enter the configuration mode for the router.

       SEFOS# configure terminal
       SEFOS(config)# router rip
       SEFOS(config-router)# network 10.0.0.1

2. Disable the passive interface status for `VLAN 1`.

       SEFOS(config-router)# no passive-interface vlan 1
       SEFOS(config-router)# exit

3. Review the RIP interface for the periodic updates sent over the interface.

       SEFOS# show ip rip statistics

       RIP Global Statistics:
       ----------------------
        Total number of route changes is 0
        Total number of queries responded is 0
        Total number of dropped packets is 0

       RIP Interface Statistics:
       -------------------------
       Interface   Periodic      BadRoutes   Triggered      BadPackets   Admin
       IP Address  Updates Sent  Received    Updates Sent   Received     Status
       ----------- ------------  ---------   ------------   ----------   ------
       10.0.0.1        1            0            0              0       Enabled

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |