Skip Navigation Links
Exit Print View
| Sun Network 10GbE Switch 72p ### User’s Guide

Search Scope:

- This Document
- Entire Library

## Connect the SER MGT Cable

The SER MGT connector is an 8-pin serial interface. You must use this connector at the physical location of the switch. This connector does not enable remote management.

1. Install the switch in the rack.

   See Install the Switch in the Rack.

2. Connect the serial management cable from the management console to the connector labeled SER MGT.
3. Configure the DHCP server with the MAC address of the management controller.

   The MAC address is printed on the (yellow) customer information sheet on the outside of the switch shipping carton.

4. Route the management cables so that they do not interfere with other cables, with servicing the switch, or with other systems.
5. Prepare the management console for communication with the management controller.
6. Power on the switch.

   See Power On the Switch.

##### Related Information

- SER MGT Port

Copyright © 2011, 2012 , Oracle and/or its affiliates. All rights reserved. Legal Notices |