Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### OSPFv3 Administration Guide

Search Scope:

- This Document
- Entire Library

### Configuring Route Calculation SPF Timers

You can configure an SPF timer to specify the delay time and hold time between two consecutive SPF calculations. Delay time is the time interval between when OSPFv3 receives a topology change and when it starts an SPF calculation. Hold time is the minimum time between two consecutive SPF calculations.

- Configure SPF Timers

- Restore the Default Delay Time

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |