Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### LLDP Administration Guide

Search Scope:

- This Document
- Entire Library

#### Default Settings

The following contains the default configuration settings for the LLDP software.

Parameter | Default Setting
--- | ---
Global Configuration Objects
System control status | Start
Module status | Disabled
Message transmit interval | 30
Hold-time multiplier | 4
Re-initialization delay | 2
Tx delay | 2
Notification interval | 5
Chassis ID subtype | MAC address
Chassis ID | MAC address of default VLAN
Port Specific Configuration Objects
Port ID subtype | Interface alias
Port ID | Interface alias of the port
Admin status | Transmit and receive (TxAndRx)
Notification status | Disabled
Notification type | Misconfiguration notification type
Optional TLVs transmission status | Disabled
Trace input | Critical trace is enabled

Optional TLVs include the following:

- Basic optional TLVs

- IEEE 802.1 organizationally-specific TLVs

- IEEE 802.3 organizationally-specific TLVs

Copyright © 2010, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |