Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### STP Administration Guide

Search Scope:

- This Document
- Entire Library

### Bridge ID and Switch Priority

Each switch has a unique bridge identifier that determines the selection of the root switch. The bridge identifier is an 8-byte field that is composed of two subfields.

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |