Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### PIMv6 Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the LAN Delay

The LAN delay, inserted by a router in the LAN prune delay option, expresses the expected message propagation delay on the interface. Upstream routers use the delay to discover the delayed time interval for a join override message before pruning an interface.

1. Associate the `VLAN 7` interface with the PIMv6 component 1.

       SEFOS(config)# interface vlan 7
       SEFOS(config-if)# ipv6 pim componentId 1
       SEFOS(config-if)# end

2. Set the LAN delay to 120 seconds on the `VLAN 7` interface.

       SEFOS# configure terminal
       SEFOS(config)# interface vlan 7
       SEFOS(config-if)# ipv6 pim lan-delay 120
       SEFOS(config-if)# end

3. Review the LAN delay value.

       SEFOS# show ipv6 pim interface detail

       vlan7 34 is up
       ...
           PIM Lan Delay: 120
       ...

Copyright © 2010, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |