Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### LLDP Administration Guide

Search Scope:

- This Document
- Entire Library

## Clear the LLDP Traffic Counters

LLDP traffic counters are updated whenever LLDP operates in transmit and receive-transmit only modes.

1. At both switches, configure the LLDP module status as enabled.

   See Configure the LLDP Module Status.

2. At both switches, enter the Global Configuration mode.

       SEFOS# configure terminal

3. Allow both switches to transmit LLDPDUs, then clear LLDP traffic counters.

       SEFOS(config)# clear lldp counters
       SEFOS(config)# end

4. On both switches, review the traffic counter values.

       SEFOS# show lldp traffic
       Total Frames Out                : 0
       Total Entries Aged                : 0
       Total Frames In                : 0
       Total Frames Received In Error        : 0
       Total Frames Discarded            : 0
       Total TLVS Unrecognized            : 0
       Total TLVs Discarded            : 0

Copyright © 2010, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |