Skip Navigation Links
Exit Print View
| Sun Ethernet Fabric Operating System ### LLDP Administration Guide

Search Scope:

- This Document
- Entire Library

## Configure the LLDP Port-ID Subtype

You can configure the port-ID subtype with any of the following values:

- Interface alias

- Port component

- MAC address

- Network address

- Intereface name

- Local

While configuring the port-ID subtype as the port component or local setting, you must provide an input string in the command for setting the port ID.

1. At both switches, configure the LLDP port ID subtype.

       SEFOS# configure terminal
       SEFOS(config)# interface extreme-ethernet 0/1
       SEFOS(config-if)# lldp port-id-subtype mac-addr
       SEFOS(config-if)# exit
       SEFOS(config)# set lldp enable
       SEFOS(config)# end

2. At switch 1, review the local system information on `extreme-ethernet 0/1`.

       SEFOS# show lldp local extreme-ethernet 0/1
       Port Id SubType            : Mac Address
       Port Id                : 00:01:02:03:04:01
       ...

3. At switch 2, review the information of the learned, remote entry on `extreme-ethernet 0/1`.

       SEFOS# show lldp neighbors extreme-ethernet 0/1 detail
       ...
       Port Id SubType            : Mac Address
       Port Id                : 00:01:02:03:04:01
       ...

Copyright © 2010, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |