Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Site Planning Guide

Search Scope:

- This Document
- Entire Library

### Environmental Specifications

The environmental specifications of the system are shown in the following table.

Specification | Operating | Nonoperating
--- | --- | ---
Temperature | 5 to 32o C (41 to 90 oF) noncondensing | –40 to 65o C (–40 to 149o F) noncondensing
Optimum ambient temperature | 22o C (71.6o F) |
Relative humidity (RH) | 10 to 90% RH, noncondensing, 27o C max wet bulb | 5 to 93% RH, noncondensing, 38o C max wet bulb
Optimum ambient relative humidity | 45 to 50% RH, noncondensing |
Altitude | 0 to 10,000 feet (3048 m) maximum ambient temperature is derated by 1o C per 300 m (984 ft) above 900 m (2953 ft) | 0 to 39,370 feet (12,000 m)
Sine vibration | Operating: Z (vertical) axis: 0.15 G, X-Y axis: 0.10 G, 5 Hz-500 Hz sine | Z (vertical) axis: 0.50 G, X-Y axis: 0.25 G, 5 Hz-500 Hz sine
Shock | 3 Gs, 11 msec, half sine (rackmounted enclosure) |

Copyright © 2008, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |