Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Service Manual

Search Scope:

- This Document
- Entire Library

## Remove an Internal Power Cable

Note - The internal power cable must be replaced only by Oracle Service personnel.

1. Power off the installed server modules and the chassis.

   Refer to the documentation for the server modules and see Power Off the Chassis and Powering Off the System and Components.

2. Remove all the modules or filler panels that are installed in the chassis.

   See Replacing Customer-Replaceable Units.

3. Remove the midplane from the chassis.

   See Remove the Midplane.

4. Locate the power cable that you need to remove.
5. Remove the retention clip and grounding clip holding the cable in the chassis housing.
6. Pull the cable downward to release it from the chassis cable housing.
7. Unfasten the cable from the metal tabs that secure it to the chassis wall.
8. Unscrew the small panel on the right rear side of the chassis.
9. Remove the two terminal clips that correspond to the power cable that you are removing.
10. Using a nut driver, remove the chassis ground connectors that correspond to the power cable that you are removing.
11. Remove the cable from the chassis.

##### Related Information

- Install an Internal Power Cable

Copyright © 2007, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |