Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Site Planning Guide

Search Scope:

- This Document
- Entire Library

#### Grid Redundancy

You can configure the Sun Blade 6000 modular system for grid redundancy by using two AC line feeds and the appropriate modular power system. Grid redundancy refers to the performance of the chassis power subsystem in the intended AC configuration. For grid redundancy, the AC configuration is supplied by AC power from two independent feeds, which can be called Line A and Line B. When you connect one power supply to the Line A feed and one power supply to the Line B feed, the system can tolerate the failure of one power supply or the complete loss of either AC feed.

Copyright © 2008, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |