Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Service Manual

Search Scope:

- This Document
- Entire Library

## Remove the Midplane

Note - The midplane must be replaced only by Oracle Service personnel.

1. Power off the installed server modules and the chassis.

   Refer to the documentation for the server modules and see Powering Off the System and Components.

2. Remove all the modules and filler panels that are installed in the chassis.

   See Replacing Customer-Replaceable Units.

3. Remove the air duct by unfastening the snaps from underneath the power supply cage and tilting the front of the air duct downward to free it from the chassis.
4. Loosen the 13 captive screws attaching the midplane to the back of the chassis.

   | Caution - Do not touch the connectors on the midplane. You might damage or bend the connector pins.

5. Pull the midplane away from the chassis guide pins, then down to clear the power supply cage.
6. Tilt the midplane slightly to the side, and remove it from the chassis.

##### Related Information

- Install the Midplane

Copyright © 2007, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |