Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Site Planning Guide

Search Scope:

- This Document
- Entire Library

#### Power Consumption

The amount of power that the system consumes dependents on its configuration, that is, the number of active modular components installed. To determine the power redundancy requirements, you need to know:

- Source power available

- Power consumption (depends on component configuration)

- Redundancy level required

The system requires a minimum of four AC inputs. To provide 2N power redundancy at a 5600W consumption level, and to ensure that the system can tolerate a loss of one power supply, the system should never exceed 6250W of power consumption at any given time.

Copyright © 2008, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |