Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Site Planning Guide

Search Scope:

- This Document
- Entire Library

### Clearance for Service and Aisle Requirements

To enable installation and servicing of the system, including access to system cables, follow these space restrictions.

Location | Service Access Requirement
--- | ---
System extended from rack | 3 feet (0.9 m) on both sides of the system to facilitate installation
Front cold aisle | 5 feet (1.5 m); required for rackmounting
Back hot aisle | 3 feet (0.9 m); required for cable access

Arrange racks in a hot aisle–cold aisle layout. This layout enables cool air to flow through the aisles to the system’s front air intake and enables heated air to flow from the system’s back exhaust. A hot aisle–cold aisle layout eliminates the direct transfer of hot exhaust air from one system into the intake air of another system.

Copyright © 2008, 2012, Oracle and/or its affiliates. All rights reserved. Legal Notices |