Skip Navigation Links
Exit Print View
| Sun Blade 6000 Modular System ### Service Manual

Search Scope:

- This Document
- Entire Library

## Install an Internal Power Cable

1. Replace the connector end of the cable in the chassis cable housing.
2. Replace the grounding clip and retention clip.
3. Route the cable through the tabs on the back wall of the chassis.
4. Route the end wires to the cable housing on the right rear of the chassis.
5. Connect the two terminal and two ground wires to the terminal and ground connectors.
6. Replace the side panel.
7. Replace all of the components that were removed from the chassis.

   See Replacing Customer-Replaceable Units and Replacing the Midplane.

8. Power on the chassis.

   See Returning the Modular System to Operation.

##### Related Information

- Returning the Modular System to Operation

- Verify Modular System Functionality

Copyright © 2007, 2013, Oracle and/or its affiliates. All rights reserved. Legal Notices |